PR: 10/2016

SICAM, Pordenone 18th - 21st October 2016

**Dial Lock 60 combination lock: new addition to the Lehmann range**

High security and robustness for heavy-duty usage applications

**Keyless security is the latest trend in lock solutions. In public areas and industrial installations, especially for lockers and deposit boxes, keyless access is one of the security requirements. Lehmann, the lock specialist based in Minden, Germany, now offers the „Dial Lock 60“ – specifically developed for heavy-duty usage applications.**

The new „Dial Lock 60“ features a special fibre-glass reinforced precision plastic casing and robust zinc diecast interior lock mechanism was designed for areas in which cabinets, lockers or deposit boxes are subject to heavy-duty usage. With a stamping configuration of 16 x 19 mm, the new „Dial Lock“ model is perfect suitable for the specific requirements of steel furniture manufacturers in mind. An adaptation is available for wood / HPL applications. Three-point locking can be realized in particularly sensitive areas (laboratories) with this combination lock.

As with all combination lock models, the „Dial Lock 60“ is also fitted with the convenient scrambling feature, which automatically resets the number dials to zero when closing. This convenient function frees the users from having to conceal the code themselves and ensures that the personal code set remains confidential.

„Dial Lock 60“ is a lock and handle in one, making the use of additional handle elements unnecessary. The ergonomically shaped knob offers good grip, enabling the user to open and close cabinets and lockers easily. Because all four number wheels reliably engage, the „Dial Lock 60“ can even be operated when wearing (work)gloves.

In case of a forgotten code, the lock can be opened via the emergency opening cylinder (Z90). The lock can be adjusted easily for application on left and right hand doors (change of clockwise / anti-clockwise of rotation). Upward and downward directions are also possible if required for specific applications, such as lift-up doors or drawers. The cam rotation is just 90°, ensuring suitability for applications with limited space.

„Dial Lock 60“ is suitable for material thicknesses up to 12 mm. The adaptation for mounting in wood enables material thicknesses from 16 to 21 mm.

Caption 1: "Dial Lock 60" is a lock and handle in one, making the use of additional handle elements unnecessary. The ergonomically shaped knob offers good grip, enabling the user to open and close cabinets and lockers easily. The lock is available in black or white. Photo: Lehmann

Caption 2: Keyless security is the latest trend, especially for lockers and deposit boxes. With a fibre-glass reinforced housing, the "Dial Lock 60" was developed specifically for heavy-duty usage. Photo: Lehmann